*******************************************************************************
*******************************************************************************
     Readme File for STT of the X-Ray Telescope Advanced Example
*******************************************************************************
*******************************************************************************

STT testing of XrayTel should contain the following:

gmake
XrayTel test.mac

this should produce one output file:
xraytel.out (0.5 kbytes)

This should be compared with 
xraytel_ref.out

The job should take ~ 2 minutes on a 1 GHz Linux machine

The memory usage should be around 6 Mbytes.

Platforms to be tested on:
SUN and LINUX, NOT WINDOWS.

At a future date G4ANALYSIS_USE should be set and the AIDA/Anaphe 
packages tested.
In this case 
- computation time ~ 4 minutes
- memory usage ~ 18 Mbytes
- the file xraytel.hbook is created (~250 kbytes)
- this file should be compared to xraytel_ref.hbook

If G4ANALYSIS_USE_PLOTTER is set together with G4ANALYSIS_USE, the 
AIDA/Anaphe plotter (Grace) can be tested in interactive runs.

Giovanni Santin
e-mail: giovanni.santin@cern.ch

*******************************************************************************
*******************************************************************************
